# 1 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
;ls_zg60
;LCC LS version 2001/03/08
;from zg30
;avance-version (10/02/09)
;1D sequence
;using 60 degree flip angle
;
;$CLASS=HighRes
;$DIM=1D
;$TYPE=
;$SUBTYPE=
;$COMMENT=
;$RECOMMEND=y


# 1 "/opt/topspin3.0/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance3.incl
;   for AV III
;
;avance-version (07/12/14)
;
;$CLASS=HighRes Incl
;$COMMENT=
# 165 "/opt/topspin3.0/exp/stan/nmr/lists/pp/Avance.incl"
;$Id: Avance3.incl,v 1.9 2009/07/02 16:40:43 ber Exp $
# 16 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60" 2


# 19 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
"acqt0=-p1*2*0.66/3.1416"


# 1 "mc_line 22 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60 exp. def. part of mc cmd. before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.333333*30m"
"MCREST = 30m - 30m"

    dccorr
# 22 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
1 ze
# 1 "mc_line 22 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60 exp. def. of mc cmd. after ze"
# 23 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
# 1 "mc_line 23 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60 exp. start label for mc cmd."
2 MCWRK  * 2
LBLF0, MCWRK
  MCREST
# 24 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
  d1
  p1*0.66 ph1
  go=2 ph31
# 1 "mc_line 27 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60 exp. mc cmd. in line"
  MCWRK wr #0
  MCWRK zd
  lo to LBLF0 times td0

  MCWRK
# 28 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
exit
# 31 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1


;pl1 : f1 channel - power level for pulse (default)
;p1 : f1 channel -  90 degree high power pulse
;d1 : relaxation delay; 1-5 * T1
;NS: 1 * n, total number of scans: NS * TD0
# 42 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zg60"
;$Id: zg30,v 1.10.2.1 2010/02/10 16:30:11 ber Exp $
