# 1 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60"
;ls_zgdc60
;LCC LS version 2013/09/12
;from zgdc30
;avance-version (07/04/03)
;1D sequence with decoupling
;using 60 degree flip angle
;
;$CLASS=HighRes
;$DIM=1D
;$TYPE=
;$SUBTYPE=
;$COMMENT=


# 1 "/opt/topspin2.1/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance2.incl
;   for 1
;
;avance-version (09/07/02)
;
;$CLASS=HighRes Incl
;$COMMENT=


















































































































































;$Id: Avance2.incl,v 1.17.2.2 2009/11/18 11:19:58 ber Exp $
# 15 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60" 2



"d11=30m"


"acqt0=-p1*2*0.66/3.1416"


# 1 "mc_line 24 file /opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60 expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.333333*30m"
"MCREST = 30m - 30m"
    dccorr
# 24 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60"
1 ze
# 1 "mc_line 24 file /opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60 expanding definition of mc command after ze"
# 25 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60"
  d11 pl12:f2 
# 1 "mc_line 26 file /opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60 expanding start label for mc command"
2 MCWRK  * 2 do:f2
LBLF0, MCWRK 
  MCREST
# 27 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60"
  d11 cpd2:f2
  d1
  p1*0.66 ph1
  go=2 ph31
# 1 "mc_line 31 file /opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60 expanding mc command in line"
  MCWRK do:f2 wr #0
  MCWRK zd 
  lo to LBLF0 times td0

  MCWRK
# 32 "/opt/topspin2.1/exp/stan/nmr/lists/pp/user/ls_zgdc60"
exit


ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1


;pl1 : f1 channel - power level for pulse (default)
;pl12: f2 channel - power level for CPD/BB decoupling
;p1 : f1 channel -  90 degree high power pulse
;d1 : relaxation delay; 1-5 * T1
;d11: delay for disk I/O                             [30 msec]
;NS: 1 * n, total number of scans: NS * TD0
;cpd2: decoupling according to sequence defined by cpdprg2
;pcpd2: f2 channel - 90 degree pulse for decoupling sequence



;$Id: zgdc30,v 1.10 2007/04/11 13:34:31 ber Exp $
