# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60"
;zg60
;avance-version (02/05/31)
; F. LACASSIN   modified 2005/07/21 15:46:37  for LS_LCC
;1D sequence
;using 60 degree flip angle


# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance2.incl
;   for 1
;
;avance-version (03/02/17)





















































































































;$Id: Avance2.incl,v 1.7.2.3 2003/02/25 14:48:48 ber Exp $
# 8 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60" 2



# 1 "mc_line 11 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60 expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.500000*30m"
"MCREST = 30m - 30m"
# 11 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60"
1 ze
# 1 "mc_line 11 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60 expanding definition of mc command after ze"
# 12 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60"
# 1 "mc_line 12 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60 expanding start label for mc command"
2 MCWRK  * 2
LBLF0, MCREST
# 13 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60"
  d1
  p1*0.66 ph1
  go=2 ph31
# 1 "mc_line 16 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60 expanding mc command in line"
  MCWRK wr #0
  MCWRK zd 
  lo to LBLF0 times td0

# 17 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60"
exit


ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1


;pl1 : f1 channel - power level for pulse (default)
;p1 : f1 channel -  90 degree high power pulse
;d1 : relaxation delay; 1-5 * T1
;NS: 1 * n, total number of scans: NS * TD0



;$Id: zg60,v 1.2 2005/07/20 14:08:06  ber Exp $

