# 1 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
;ls_zgdc60 LS version
; from zgdc30
;avance-version (07/04/03)
;1D sequence with decoupling
;using 60 degree flip angle
;
;$CLASS=HighRes
;$DIM=1D
;$TYPE=
;$SUBTYPE=
;$COMMENT=


# 1 "/opt/topspin3.0/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance3.incl
;   for AV III
;
;avance-version (07/12/14)
;
;$CLASS=HighRes Incl
;$COMMENT=
# 165 "/opt/topspin3.0/exp/stan/nmr/lists/pp/Avance.incl"
;$Id: Avance3.incl,v 1.9 2009/07/02 16:40:43 ber Exp $
# 14 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60" 2


# 17 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
"d11=30m"


"acqt0=-p1*2*0.66/3.1416"
# 1 "mc_line 23 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60 exp. def. part of mc cmd. before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.333333*30m"
"MCREST = 30m - 30m"

    dccorr
# 23 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
# 23 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
1 ze
# 1 "mc_line 23 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60 exp. def. of mc cmd. after ze"
# 24 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
  d11 pl12:f2 
# 1 "mc_line 25 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60 exp. start label for mc cmd."
2 MCWRK  * 2 do:f2
LBLF0, MCWRK 
  MCREST
# 26 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
  d11 cpd2:f2
  d1
  p1*0.66 ph1
  go=2 ph31
# 1 "mc_line 30 file /opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60 exp. mc cmd. in line"
  MCWRK do:f2 wr #0
  MCWRK zd
  lo to LBLF0 times td0

  MCWRK
# 31 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
exit


ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1
# 38 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
;pl1 : f1 channel - power level for pulse (default)
;pl12: f2 channel - power level for CPD/BB decoupling
;p1 : f1 channel -  90 degree high power pulse
;d1 : relaxation delay; 1-5 * T1
;d11: delay for disk I/O                             [30 msec]
;NS: 1 * n, total number of scans: NS * TD0
;cpd2: decoupling according to sequence defined by cpdprg2
;pcpd2: f2 channel - 90 degree pulse for decoupling sequence


# 49 "/opt/topspin3.0/exp/stan/nmr/lists/pp/user/ls_zgdc60"
;$Id: zgdc30,v 1.11 2009/07/02 16:40:47 ber Exp $
