# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb"
;zg60dcdcb
;avance-version (02/05/31)
; F. LACASSIN   modified 2005/07/20 14:33:48  for LS_LCC
;1D sequence with decoupling H/X and Y
;using f2 - and f3 - channel


# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance2.incl
;   for 1
;
;avance-version (03/02/17)





















































































































;$Id: Avance2.incl,v 1.7.2.3 2003/02/25 14:48:48 ber Exp $
# 8 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb" 2




"d11=30m"


# 1 "mc_line 15 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
"MCWRK = 0.500000*30m"
"MCREST = 30m - 30m"
# 15 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb"
1 ze
# 1 "mc_line 15 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb expanding definition of mc command after ze"
# 16 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb"
  d11 pl12:f2 pl16:f3
# 1 "mc_line 17 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb expanding start label for mc command"
2 MCWRK  * 2 cpd2:f2 cpd3:f3
LBLF0, MCREST
# 18 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb"
  d1
  p1*.66 ph1
  go=2 ph31 
# 1 "mc_line 21 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb expanding mc command in line"
  MCWRK do:f2 do:f3 wr #0
  MCWRK zd 
  lo to LBLF0 times td0

# 22 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_zg60dcdcb"
exit


ph1=0 2 2 0 1 3 3 1
ph31=0 2 2 0 1 3 3 1


;pl1 : f1 channel - power level for pulse (default)
;pl12: f2 channel - power level for CPD/BB decoupling
;pl16: f3 channel - power level for CPD/BB decoupling
;p1 : f1 channel -  high power pulse
;d1 : relaxation delay; 1-5 * T1
;d11: delay for disk I/O                             [30 msec]
;NS: 1 * n, total number of scans: NS * TD0
;cpd2: decoupling according to sequence defined by cpdprg2
;cpd3: decoupling according to sequence defined by cpdprg3
;pcpd2: f2 channel - 90 degree pulse for decoupling sequence
;pcpd3: f3 channel - 90 degree pulse for decoupling sequence



;$Id: zg60dcdcb,v 1.7 2002/06/12 09:05:22 ber Exp $
