# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc"
;ls_cosygpqfdc
;avance-version (00/04/28)
;2D homonuclear shift correlation
;using gradient pulses for selection
; F. LACASSIN   modified 2005/12/07 15:05:03  for LS_LCC
; using f2 chanel for BB decoupling


# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance2.incl
;   for 1
;
;avance-version (03/02/17)





















































































































;$Id: Avance2.incl,v 1.7.2.3 2003/02/25 14:48:48 ber Exp $
# 9 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc" 2

# 1 "/opt/xwinnmr/exp/stan/nmr/lists/pp/Grad.incl" 1
;Grad2.incl  -  include file for Gradient Spectroscopy
;   for 1
;
;avance-version (02/05/31)



















define list<gradient> EA=<EA>



;$Id: Grad2.incl,v 1.7 2002/06/12 09:04:22 ber Exp $
# 10 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc" 2




"d0=3u"

"d13=4u"


# 1 "mc_line 19 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
"MCWRK = d1"
"MCREST = d1 - d1"
# 19 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc"
1 ze
# 1 "mc_line 19 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc expanding definition of mc command after ze"
# 20 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc"
  d11 pl12:f2
  d11 cpd2:f2
# 1 "mc_line 22 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc expanding start label for mc command"
2 MCWRK 
LBLF1, MCREST
# 23 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc"
3 p1 ph1
  d0
  50u setnmr3|0 setnmr0|34|32|33
  p16:gp1
  d16
  p0 ph2
  d13
  p16:gp2
  d16
  4u setnmr3^0 setnmr0^34^32^33
  go=2 ph31
# 1 "mc_line 34 file /opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc expanding mc command in line"
  MCWRK  wr #0 if #0 zd id0 
  lo to LBLF1 times td1
# 35 "/opt/xwinnmr/exp/stan/nmr/lists/pp/ls_cosygpqfdc"
  d11 do:f2
exit


ph1=0 2
ph2=0 0 2 2
ph31=0 2


;pl1 : f1 channel - power level for pulse (default)
;pl12: f2 channel - power level for CPD/BB decoupling
;cpd2: decoupling according to sequence defined by cpdprg2
;pcpd2: f2 channel - 90 degree pulse for decoupling sequence
;p0 : f1 channel -  20 to 90 degree high power pulse
;p1 : f1 channel -  90 degree high power pulse
;p16: homospoil/gradient pulse
;d0 : incremented delay (2D)                         [3 usec]
;d1 : relaxation delay; 1-5 * T1
;d13: short delay                                    [4 usec]
;d16: delay for homospoil/gradient recovery
;in0: 1/(1 * SW) = 2 * DW
;nd0: 1
;NS: 1 * n
;DS: 16
;td1: number of experiments
;FnMODE: QF

;use gradient ratio:	gp 1 : gp 2
;			  10 :   10

;for z-only gradients:
;gpz1: 10%
;gpz2: 10%

;use gradient files:   
;gpnam1: SINE.100
;gpnam2: SINE.100



;$Id: cosygpqf,v 1.3 2002/06/12 09:04:27 ber Exp $
